|  |  |  |
| --- | --- | --- |
| **FLAG : PANAMA CALL SIGN : 3E2031 OFFICIAL NO: 54334 - PEXT** | **MMSI NO :352898741 PORT OF REGISTRY: PANAMA SAT C : 437401059** | **TELEX :** |
| **SHIP TYPE: PRODUCT OIL/CHEMICAL TANKER** | | |
| **CLASS : INTERNATIONAL REGISTER OF SHIPPING** | | |
| **CLASS NOTATION : PHRS 100AL.1MS.ESP.OILTANKER** | | |
| **OWNER: INDO PACIFIC SHIPMANAGEMENT CO. LTD.** | | |
| **ADDRESS: AJEL TAKE ROAD, AJELTAKE ISLAND, MAJURO ISLAND, MARSHALL ISLAND.** | | |
| **YEAR OF BUILD : 2006 SHIPYARD : YARDIMCI** | | |
| **HULL NO. : 048 KEEL LAID : 02 NOVEMBER 2005** | | |
| **DELIVERED : 01 NOVEMBER 2006 TEL: +971 48786410** | | |
| **DEAD SLOW SLOW HALF FULL FULL SEA** | | |
| **BALLAST 13.0 14.4 14.8 LOADED 12.5 13.8 14.1** | | |
| **LOA 118.37 m GROSS TONNAGE 6522** | | |
| **LBP 112.0 m NET TONNAGE 3220** | | |
| **PARELLEL BODY-LADEN 55.00 m SUEZ CANAL TONNAGE 5366** | | |
| **PARALLEL BODY-BALLAST 39.00 m PANAMA CANAL TONNAGE 5535** | | |
| **KEEL TO MASTHEAD 36.20 m** | | |
| **BREADTH 19.00 m DEPTH MOULDED 10.10 m ALLOWANCE FOR FRESH WATER 171** | | |
| **BRIDGE TO BOW 97.10 m ANCHOR CHAIN PS 10 shackle** | | |
| **BRIDGE TO STERN 21.27 m ANCHOR CHAIN SS 10 shackle** | | |
| **BRIDGE TO MANIFOLD 39.70 BOW TO MANIFOLD 57.30** | | |
| **STERN TO MANIFOLD 61.07 m MTC SUMMER 152.4 mt** | | |
| **MANIFOLD TO SHIP SIDE 4.40 m TPC SUMMER 19.5 mt** | | |
| **MANIFOLD ABOVE DECK 2.70 m LIGHT WEIGHT 3741.1 mt** | | |
|  | | |
| **FREEBOARD DARFT MLD DEADWEIGHT DISPLACEMENT** | | |
| **LOADLINE (m) (m) (m) (m)** | | |
| **SUMMER 1.891 8.221 9971.1 13712.1** | | |
| **WINTER 2.062 8.050 9637.1 13378.1** | | |
| **TROPICAL 1.720 8.392 10307.3 14048.3** | | |
| **FRESH WATER 1.720 8.392 9964.6 13705.6** | | |
| **TFW 1.548 8.564 10296.5 14037.5** | | |